**Load Adjustment Factors**

# **Importance factor**

**Risk 1: Uninhabited (For example, a warehouse, storage, etc.) – 0.8**

**Risk 2: All other structures – 1.0**

**Risk 3: Important (For example, hospitals, schools) – 1.1**

**Risk 4: Critical (For example, a disaster shelter, nuclear power plant, etc.) – 1.2**

# **Heating factor**

**Unheated building (warehouse, garage, etc.) – 1.2**

**Heated greenhouse – 0.85**

**All other structures – 1.0**

# **Exposure factor**

**Fully exposed – 0.9**

**Partially exposed – 1.0**

**Sheltered – 1.2**